## Add Apply Offset option in vtkPDALReader

`vtkPDALReader` now exposes an **Apply Offset** property in ParaView.
When enabled, offsets detected in LAS/LAZ metadata are applied to point coordinates on read.

![Apply Offset option image](apply-offset-option-pdalreader.png)
