Specify TEM3P - Thermal
========================

At this point, all of the elastic specifications are complete. So next we complete the thermal specifications.


.. Apply class for custom formatting of numbered steps.
.. rst-class:: step-number

1\. TEM3P Thermal - Boundary Conditions Tab

Select the :guilabel:`TEM3P Thermal` tab and underneath that select the :guilabel:`Boundary Conditions` tab. Set the boundary condition types and data items per this table and screenshot:

::

  Side Set    Type        Item Name             Item Value
  ----------------------------------------------------------------------
      1      Neumann      Heat Flux                   0
  ----------------------------------------------------------------------
      2      Neumann      Heat Flux                   0
  ----------------------------------------------------------------------
      3      Neumann      Heat Flux                   0
  ----------------------------------------------------------------------
      4      Neumann      Heat Flux                   0
  ----------------------------------------------------------------------
      5       Robin       Robin Constant Factor   20000
                          Robin Constant Value   440000
  ----------------------------------------------------------------------
      6     RF Heating    use the values shown in the screenshot below
  ----------------------------------------------------------------------


.. image:: images/rfgun-boundary-conditions2b.png
    :align: center


.. Apply class for custom formatting of numbered steps.
.. rst-class:: step-number

2\. TEM3P Thermal - Materials Tab

Under the :guilabel:`TEM3P Thermal` tab select the :guilabel:`Materials` tab. Add a material attribute by clicking the :guilabel:`New` button, set the :guilabel:`Thermal Conductivity` to ``391``, and assign ``Unnamed Block ID: 1`` to the :guilabel:`Current` list.

.. image:: images/rfgun-materials2b.png
    :align: center

|

.. Apply class for custom formatting of numbered steps.
.. rst-class:: step-number

3\. TEM3P Thermal - Analysis Tab

In the :guilabel:`Analysis` tab, set the parameters as shown in this screenshot:

.. image:: images/rfgun-analysis2b.png
    :align: center

|
