![SLAM in LidarView](doc/paraview_plugin.png)

![SLAM in ROS](doc/ros_node.png)

# LiDAR SLAM

- [Introduction and contents](#introduction-and-contents)
- [Core SLAM lib](#core-slam-lib)
  - [Dependencies](#dependencies)
  - [Installation](#installation)
- [ROS wrapping](#ros-wrapping)
  - [Dependencies](#dependencies-1)
  - [Installation](#installation-1)
  - [Usage](#usage)
- [ParaView wrapping](#paraview-wrapping)
  - [Dependencies](#dependencies-2)
  - [Installation](#installation-2)
  - [Usage](#usage-1)
  - [Use SLAM in LidarView](#use-slam-in-lidarview)

## Introduction and contents

This repo contains LiDAR-only visual SLAM developped by Kitware, as well as ROS and ParaView wrappings for easier use.

It has been successfully tested on data from several common LiDAR sensors:
- Velodyne (VLP-16, VLP-32c, HDL-32, HDL-64, VLS-128)
- Ouster (OS0/1/2-32/64/128)
- RoboSense (RS-LiDAR-16 RS-LiDAR-32)
- Hesai (PandarXT16, PandarXT32, Pandar128)

Have a look at our [SLAM demo video](https://vimeo.com/524848891)!

This codebase is under active development. If you're interested by new features, new sensors' support or any project that could be using this SLAM, do not hesitate to contact us at kitware@kitware.com.

Repo contents :
- `slam_lib/` : core *LidarSlam* library containing SLAM algorithm and other utilities.
- `superbuild/` : Cross-platform installer.
- `ros_wrapping/` : ROS packages to enable SLAM use on a ROS system.
- `paraview_wrapping/` : ParaView plugin to enable SLAM use with ParaView/LidarView.
- `ci/` : continuous integration files to automatically build and check *LidarSlam* lib.
- `CMakeLists.txt` : *CMakeLists* used to call to build core *LidarSlam* lib and *paraview_wrapping*.

## Core SLAM lib

### Dependencies

Dependencies are listed in the table below along with the version used during development and testing. Minimum required versions have not been determined yet.

| Dependency | Minimum tested Version |
| :--------: | :--------------------: |
| Eigen3     | 3.3.4                  |
| Ceres      | 1.13.0                 |
| PCL        | 1.8                    |
| nanoflann  | 1.3.0                  |
| g2o*       | 1.0.0 (master)         |
| OpenMP*    | 2.0                    |
| gtsam*     | 4.2a8                  |
| OpenCV*    | 4.5.4                  |

(*) optional dependencies :

- If G2O is not available (or disabled), *LidarSlam* lib will still be compiled, but without pose graph optimization features.
- If GTSAM is not available (or disabled), *LidarSlam* lib will still be compiled, but without IMU processing features.
- If OpenCV is not available (or disabled), *LidarSlam* lib will still be compiled, but without camera features.
- If OpenMP is available, it is possible to use multi-threading to run some SLAM steps in parallel and achieve higher processing speed.
- If OpenCV is not available (or disabled), *LidarSlam* lib will still be compiled, but without camera integration.

**/!\ Warning** Make sure to compile/install G2O with the same Ceres version as the one used in the SLAM compilation. To do so, disable the feature [G2O_USE_VENDORED_CERES](https://github.com/RainerKuemmerle/g2o/blob/master/CMakeLists.txt) during G2O compilation and link against the right version of Ceres.

### Installation

The *LidarSlam* lib has been tested on Linux, Windows and OS X.

First, got to your workspace directory and clone the SLAM repository.
```bash
git clone https://gitlab.kitware.com/keu-computervision/slam.git src --recursive
```

#### With system dependencies

To build only *LidarSlam* lib using your system dependencies, run :

```bash
mkdir build && cd build
cmake ../src -DCMAKE_BUILD_TYPE=Release
cmake --build . -j
```

**NOTE** : On Windows, if some dependencies were installed using vcpkg, the variable `CMAKE_TOOLCHAIN_FILE` must be specified :
cmake ../src -DCMAKE_BUILD_TYPE=Release -DCMAKE_TOOLCHAIN_FILE=[vcpkg-install]/scripts/buildsystems/vcpkg.cmake

#### With local dependencies

You can link to the local libraries you have installed adding cmake flags. Notably with Ceres and G2O:
```bash
cmake ../src -DCMAKE_BUILD_TYPE=Release -DCeres_DIR=path/to/CeresConfig.cmake -Dg2o_DIR=path/to/g2oConfig.cmake
```

#### With Superbuild

In your workspace, run :

```bash
mkdir build && cd build
cmake ../src/slam-superbuild -DCMAKE_BUILD_TYPE=Release
cmake --build . -j
```

**NOTE**: By default in the superbuild, mandatory dependencies are installed but optional dependencies are not. You can decide which dependencies to install with the superbuild using the options **INSTALL_XX**. For example, to not build *PCL*:
```bash
cmake ../src/slam-superbuild -DCMAKE_BUILD_TYPE=Release -DINSTALL_PCL=OFF
```

Note that installing and enabling an optional dependency is not the same. If you want to install and enable the use of an optional dependency you need to switch two variables to ON : **INSTALL_XX** and **ENABLE_XX**.

Example for *GTSAM* :
```bash
cmake ../src/slam-superbuild -DCMAKE_BUILD_TYPE=Release -DINSTALL_GTSAM=ON -DENABLE_GTSAM=ON
```

More documentation about the superbuild can be found [here](https://gitlab.kitware.com/keu-computervision/slam-superbuild).

## ROS wrapping

The ROS wrapping has been tested on Linux only.

### Dependencies

Ensure all *LidarSlam* dependencies are respected. Specific ROS packages dependencies are listed in the table below along with the version used during development and testing.

| Dependency      | Tested Versions | Install (`sudo apt-get install <pkg>`)                                             | status    |
|:---------------:|:---------------:|:----------------------------------------------------------------------------------:|:---------:|
| ROS             | melodic, noetic | `ros-$ROS_DISTRO-desktop-full` and [tutorial](http://wiki.ros.org/ROS/Installation)| mandatory |
| pcl-ros         | 1.7.4           | `ros-$ROS_DISTRO-pcl-ros`                                                          | mandatory |
| geodesy         | 0.5.3           | `ros-$ROS_DISTRO-geodesy`                                                          | mandatory |
| gps_common      | 0.3.0           | `ros-$ROS_DISTRO-gps-common`                                                       | optionnal |
| apriltag        | 3.2.0           | `ros-$ROS_DISTRO-apriltag`                                                         | optionnal |
| g2o             | 5.3             | `ros-$ROS_DISTRO-libg2o`                                                           | optionnal |

For Velodyne usage, please note that the ROS Velodyne driver with minimum version 1.6 is needed.
Be careful, this ROS Velodyne driver 1.6 is not backward-compatible with previous versions.
If you're running on Ubuntu 20 / ROS Noetic, you can install the new Velodyne driver using the command `sudo apt install ros-noetic-velodyne ros-noetic-velodyne-pcl`.
If running on previous versions of Ubuntu/ROS (18/Melodic and below), you need to compile this driver from source : just clone the [git repo](https://github.com/ros-drivers/velodyne) in your catkin worskpace sources, it will be automatically built with next  `catkin_make` or `catkin build`.

For Ouster usage, the driver can be found in this [git repo](https://github.com/ouster-lidar/ouster_example)

### Installation

Clone this git repo directly into your workspace under the src directory
git clone https://gitlab.kitware.com/keu-computervision/slam.git src/slam --recursive

**NOTE** : Boost, g2o and PCL dependencies can be resolved wih ROS packages.
**WARNING** : Be sure to use the same PCL library dependency for ROS basic tools and slam library to avoid compilation errors and/or segfaults.

#### With system dependencies
Run `catkin_make -DCMAKE_BUILD_TYPE=RelWithDebInfo` or `catkin_make -DCMAKE_BUILD_TYPE=Release` (to turn on optimizations, highly recommended when using Eigen). The same can be done with `catkin build`. It will automatically build *LidarSlam* lib before ROS packages.

#### With local dependencies
As with Core SLAM lib, you can use local dependencies for Slam lib by passing them to catkin.

Example for Ceres and g2o :
 ```bash
 catkin_make -j -DCMAKE_BUILD_TYPE=Release --cmake-args -DCeres_DIR=path/to/CeresConfig.cmake -Dg2o_DIR=path/to/g2oConfig.cmake
  OR
 catkin build -j -DCMAKE_BUILD_TYPE=Release --cmake-args -DCeres_DIR=path/to/CeresConfig.cmake -Dg2o_DIR=path/to/g2oConfig.cmake
 ```

#### With Superbuild
The [superbuild](https://gitlab.kitware.com/keu-computervision/slam-superbuild/) can also download and install the required dependencies.

**WARNING** It is not possible to use PCL from the superbuild (this would create runtime issues with system version).

**WARNING** The superbuild must be installed outside of catkin workspace.

Example :
 ```bash
 # Clone project
 git clone https://gitlab.kitware.com/keu-computervision/slam.git catkin_ws/src/slam --recursive
 # Build Superbuild
 mkdir SB-build && cd SB-build
 cmake ../catkin_ws/src/slam/slam-superbuild -GNinja -DCMAKE_BUILD_TYPE=Release -DINSTALL_PCL=OFF
 cmake --build . -j
 # Build Slam ROS package
 cd ../catkin_ws
 catkin_make -j -DCMAKE_BUILD_TYPE=Release --cmake-args -DSUPERBUILD_INSTALL_DIR=absolute/path/to/superbuild/install
  OR
 catkin build -j -DCMAKE_BUILD_TYPE=Release --cmake-args -DSUPERBUILD_INSTALL_DIR=absolute/path/to/superbuild/install
```

### Live usage

For Velodyne :
```bash
roslaunch lidar_slam slam_velodyne.launch use_sim_time:=false
roslaunch lidar_slam slam_velodyne.launch use_sim_time:=false gps:=true   # if GPS/SLAM calibration has to be run
```

For Ouster :
```bash
roslaunch lidar_slam slam_ouster.launch replay:=false
roslaunch lidar_slam slam_ouster.launch replay:=false gps:=true   # if GPS/SLAM calibration has to be run
```

See [ros_wrapping/lidar_slam/README.md](ros_wrapping/lidar_slam/README.md) for more details.

## ParaView wrapping

The *LidarSlamPlugin* Paraview wrapping has been tested on Linux, Windows and OS X.

### Dependencies

Ensure all *LidarSlam* dependencies are respected. Specific dependencies are listed in the table below along with the version used during development and testing.

| Dependency | Tested Version    |
| :--------: | :------------:    |
| ParaView   | 5.4, 5.6 and 5.9  |

Be careful to use and link to the same libraries as ParaView/LidarView's (especially with VTK, Eigen, PCL, Ceres, nanoflann, etc.). Otherwise, if different flags or modules were enabled, some troubles may arise at build time, or it could lead to version mismatch and segfault at runtime.

For example, if PCL is built with `pcl_visualization` module, it must link to the same VTK than the one used by ParaView.

### Installation

To build *LidarSlam* lib and this ParaView plugin *LidarSlamPlugin*, just `cd` to this repo root dir and run :

```bash
mkdir build
cd build
cmake .. -DCMAKE_BUILD_TYPE=RelWithDebInfo -DSLAM_PARAVIEW_PLUGIN:BOOL=ON
cmake --build . -j
```

Set XX_DIR variables to the same path dependencies of ParaView/LidarView when they exist (Eigen, Ceres, nanoflann, etc...).

### Usage

- Open ParaView
- **Tools** tab > **Manage Plugins** > **Load New**
- Browse to the `<install>/lib/` dir and select `libLidarSlamPlugin.so` or `LidarSlamPlugin.dll`
- Load LiDAR frames and LiDAR calibration to use
- Select the frames in the Pipeline Browser, instantiate a SLAM filter, and apply it.

Currently, all features are not available in ParaView plugin. Features such as GPS/LiDAR calibration, pose graph optimization or temporal logging are only supported in ROS wrapping. However, ParaView plugin is useful to play with SLAM, interactively try out parameters, visualize and export results.

### Use SLAM in LidarView

This *LidarSlamPlugin* is natively included in [LidarView](https://www.paraview.org/lidarview/). For more detailed information on how to enable and use SLAM filter in LidarView, see [paraview_wrapping/Plugin/doc/How_to_SLAM_with_LidarView.md](paraview_wrapping/Plugin/doc/How_to_SLAM_with_LidarView.md).

Pre-built binaries of LidarView with this SLAM plugin are available for download [here](https://gitlab.kitware.com/LidarView/lidarview/-/releases).
