### Description
This example demonstrates how to setup a source that produces two outputs. The output on port 0 is of type vtkTestA and the Value gets set to 111. The output on port 1 is of type vtkTestB and the Value gets set to 222.
