### Description
The discrete Fourier transform changes an image from the spatial domain into the frequency domain, where each pixel represents a sinusoidal function. This example shows an image and its power spectrum displayed using a logarithmic transfer function.
