Converting Existing Systems To CMake
************************************

For many people, the first thing they will do with CMake is convert an
existing project from using an older build system to use CMake. This
can be a fairly easy process, but there are a few issues to
consider. This section will address those issues and provide some
suggestions for effectively converting a project over to CMake. The
first issue to consider when converting to CMake is the project's
directory structure.

.. index::
   single: directory structure

Source Code Directory Structures
================================

Most small projects will have their source code in either the top
level directory or in a directory named ``src`` or ``source``. Even if
all of the source code is in a subdirectory, we highly recommend
creating a CMakeLists file for the top level directory. There are two
reasons for this. First, it can be confusing to some people that they
must run CMake on the subdirectory of the project, instead of the main
directory. Second, you may want to install documentation or other
support files from the other directories. By having a CMakeLists file
at the top of the project, you can use the :command:`add_subdirectory`
command to step down into the documentation directory where its
CMakeLists file can install the documentation (you can have a
CMakeLists file for a documentation directory with no targets or
source code).

For projects that have source code in multiple directories, there are
a few options. One option that many Makefile-based projects use is to
have a single Makefile at the top-level directory that lists all the
source files to compile in their subdirectories. For example::

 SOURCES=\
   subdir1/foo.cxx \
   subdir1/foo2.cxx \
   subdir2/gah.cxx \
   subdir2/bar.cxx

This approach works just as well with CMake using a similar syntax::

 set(SOURCES
   subdir1/foo.cxx
   subdir1/foo2.cxx
   subdir1/gah.cxx
   subdir2/bar.cxx
   )

Another option is to have each subdirectory build a library or
libraries that can then be linked into the executables. In those
cases, each subdirectory would define its own list of source files and
add the appropriate targets. A third option is a mixture of the first
two; each subdirectory can have a CMakeLists file that lists its
sources, but the top-level CMakeLists file will not use the
:command:`add_subdirectory` command to step into the subdirectories. Instead,
the top-level CMakeLists file will use the :command:`include` command to
include each of the subdirectory's CMakeLists files. For example, a
top-level CMakeLists file might include the following code

.. index::
   single: command ; add_executable
   single: command ; endforeach
   single: command ; foreach
   single: command ; set

::

 # collect the files for subdir1
 include(subdir1/CMakeLists.txt)
 foreach(FILE ${FILES})
   set(subdir1Files ${subdir1Files} subdir1/${FILE})
 endforeach()

 # collect the files for subdir2
 include(subdir2/CMakeLists.txt)
 foreach(FILE ${FILES})
   set(subdir2Files ${subdir2Files} subdir2/${FILE})
 endforeach()

 # add the source files to the executable
 add_executable(foo ${subdir1Files} ${subdir2Files})

While the CMakeLists files in the subdirectories might look like the
following::

 # list the source files for this directory
 set(FILES
   foo1.cxx
   foo2.cxx
   )

The approach you use is entirely up to you. For large projects, having
multiple shared libraries can certainly improve build times when
changes are made. For smaller projects, the other two approaches have
their advantages. The main suggestion here is to choose a strategy and
stick with it.

.. index::
   single: in-source build
   single: out-of-source build
   single: Visual Studio

Build Directories
=================

The next issue to consider is where to put the resulting object files,
libraries, and executables. There are a few different, commonly used
approaches, and some work better with CMake than others. The recommended
strategy is to put the binary files into a separate tree that has the
same structure as the source tree. For example, if the source tree looked
like the following::

 foo/
   subdir1
   subdir2

the binary tree might look like::

 foobin/
   subdir1
   subdir2

For some Windows generators, such as Visual Studio, build files are
actually kept in a subdirectory matching the selected configuration; e.g.
debug, release, etc.

If you need to support multiple architectures from one source tree, we highly
recommend a directory structure like the following::

 projectfoo/
   foo/
     subdir1
     subdir2
   foo-linux/
     subdir1
     subdir2
   foo-osx/
     subdir1
     subdir2
   foo-solaris/
     subdir1
     subdir2

That way, each architecture has its own build directory and will not
interfere with any other architecture. Remember that not only are the
object files kept in the binary directories, but also any configured
files that are typically written to the binary tree. Another tree
structure found primarily on UNIX projects is one where the binary
files for different architectures are kept in subdirectories of the
source tree (see below). CMake does not work well with this structure,
so we recommend switching to the separate build tree structure shown
above.

::

 foo/
   subdir1/
     linux
     solaris
     hpux
   subdir2/
     linux
     solaris
     hpux

CMake provides three variables for controlling where binary targets
are written. They are the :variable:`CMAKE_RUNTIME_OUTPUT_DIRECTORY`,
:variable:`CMAKE_LIBRARY_OUTPUT_DIRECTORY`, and
:variable:`CMAKE_ARCHIVE_OUTPUT_DIRECTORY` variables. These variables are used
to initialize properties of libraries and executables to control where
they will be written. Setting these enables a project to place all the
libraries and executables into a single directory. For projects with
many subdirectories, this can be a real time saver. A typical
implementation is shown below::

 # Setup output directories.
 set(CMAKE_RUNTIME_OUTPUT_DIRECTORY ${PROJECT_BINARY_DIR}/bin)
 set(CMAKE_LIBRARY_OUTPUT_DIRECTORY ${PROJECT_BINARY_DIR}/lib)
 set(CMAKE_ARCHIVE_OUTPUT_DIRECTORY ${PROJECT_BINARY_DIR}/lib)

.. index::
   single: Windows ; build directory

In this example, all the "runtime" binaries will be written to the
``bin`` subdirectory of the project's binary tree, including
executable files on all platforms and DLLs on Windows.  Other binaries
will be written to the ``lib`` directory.  This approach is very
useful for projects that make use of shared libraries (DLLs) because
it collects all of the shared libraries into one directory. If the
executables are placed in the same directory, then they can find the
required shared libraries more easily when run on Windows.

One final note on directory structures: with CMake, it is perfectly
acceptable to have a project within a project. For example, within the
Visualization Toolkit's source tree is a directory that contains a
complete copy of the zlib compression library. In writing the
CMakeLists file for that library, we use the :command:`project` command to
create a project named VTKZLIB even though it is within the VTK source
tree and project. This has no real impact on VTK, but it does allow us
to build zlib independent of VTK without having to modify its
CMakeLists file.

Useful CMake Commands When Converting Projects
==============================================
.. index::
   single: command ; add_executable
   single: command ; file
   single: file ; globbing

There are a few CMake commands that can make the job of converting an
existing project easier and faster. The :command:`file` command with the
``GLOB`` argument allows you to quickly set a variable containing a
list of all the files that match the glob expression. For example::

 # collect up the source files
 file(GLOB SRC_FILES "*.cxx")

 # create the executable
 add_executable(foo ${SRC_FILES})

will set the ``SRC_FILES`` variable to a list of all the ``.cxx``
files in the current source directory. It will then create an
executable using those source files. Windows developers should be
aware that glob matches are case sensitive.

.. index::
   single: converting MakeFiles to CMake

Converting UNIX Makefiles
=========================

If your project is currently based on standard UNIX Makefiles then their 
conversion to CMake should be fairly straightforward. Essentially, for every 
directory in your project that has a Makefile, you will create a matching
CMakeLists file. How you handle multiple Makefiles in a directory
depends on their function. If the additional Makefiles (or Makefile
type files) are simply included in the main Makefile, you can create
matching CMake input (.cmake) files and include them into your main CMakeLists
file in a similar manner. If the different Makefiles are meant to be
invoked on the command line for different situations, consider
creating a main CMakeLists file that uses some logic to choose which
one to :command:`include` based on a CMake option.

Frequently Makefiles have a list of object files to compile. These can be
converted to CMake variables as follows::

 OBJS= \
   foo1.o \
   foo2.o \
   foo3.o

becomes

::

 set(SOURCES
   foo1.c
   foo2.c
   foo3.c
 )

While the object files are typically listed in a Makefile, in CMake
the focus is on the source files. If you used conditional statements
in your Makefiles, they can be converted over to CMake :command:`if`
commands. Since CMake handles generating dependencies, most
dependencies or rules to generate dependencies can be
eliminated. Where you have rules to build libraries or executables,
replace them with :command:`add_library` or :command:`add_executable`
commands.

Some UNIX build systems (and source code) make heavy use of the
system architecture to determine which files to compile or what flags to
use. Typically this information is stored in a Makefile variable
called ``ARCH`` or ``UNAME``. The first choice in these cases is to replace 
the architecture-specific code with a more generic test. With some software 
packages, there is too much architecture specific code for such a change to be
reasonable, or you may want to make decisions based on architecture
for other reasons. In those cases, you can use the variables
:variable:`CMAKE_SYSTEM_NAME` and :variable:`CMAKE_SYSTEM_VERSION`. They 
provide fairly detailed information on the operating system and version of 
the host computer.

.. index::
   single: autoconf ; converting to CMake
   single: converting autoconf projects to CMake

Converting Autoconf Based Projects
==================================

Autoconf-based projects primarily consist of three key pieces. The
first is the configure.in file which drives the process. The second is
Makefile.in which will become the resulting Makefile, and the third
piece is the remaining configured files that result from running
configure. In converting an autoconf based project to CMake, start
with the configure.in and Makefile.in files.

The Makefile.in file can be converted to CMake syntax as explained in
the preceding section on converting UNIX Makefiles. Once this has been
done, convert the configure.in file into CMake syntax. Most functions
(macros) in autoconf have corresponding commands in CMake. A short
table of some of the basic conversions is listed below:

**AC_ARG_WITH**
  Use the :command:`option` command.

**AC_CHECK_HEADER**
  Use the ``check_include_file`` macro from the :module:`CheckIncludeFile`
  module.

**AC_MSG_CHECKING**
  Use the :command:`message` command with the ``STATUS`` argument.

**AC_SUBST**
  Done automatically when using the :command:`configure_file` command.

**AC_CHECK_LIB**
  Use the ``check_libary_exists`` macro from the
  :module:`CheckLibraryExists` module.

**AC_CONFIG_SUBDIRS**
  Use the :command:`add_subdirectory` command.

**AC_OUTPUT**
  Use the :command:`configure_file` command.

**AC_TRY_COMPILE**
  Use the :command:`try_compile` command.

If your configure script performs test compilations using
``AC_TRY_COMPILE``, you can use the same code for CMake. Either put it
directly into your CMakeLists file if it is short, or preferably put
it into a source code file for your project. We typically put such
files into a CMake subdirectory for large projects that require such
testing.

Where you are relying on autoconf to configure files, you can use
CMake's :command:`configure_file` command. The basic approach is the same and
we typically name input files to be configured with a ``.in``
extension just as autoconf does. This command replaces any variables
in the input file referenced as ``${VAR}`` or ``@VAR@`` with their
values as determined by CMake. If a variable is not defined, it will
be replaced with nothing. Optionally, only variables of the form
``@VAR@`` will be replaced and ``${VAR}`` will be ignored. This is
useful for configuring files for languages that use ``${VAR}`` as a
syntax for evaluating variables. You can also conditionally define
variables using the C pre processor by using ``#cmakedefine VAR``. If
the variable is defined then :command:`configure_file` will convert the
``#cmakedefine`` into a ``#define``; if it is not defined, it will
become a commented out ``#undef``. For example::

 /* what byte order is this system */
 #cmakedefine CMAKE_WORDS_BIGENDIAN

 /* what size is an INT */
 #cmakedefine SIZEOF_INT @SIZEOF_INT@

.. index::
   single: converting Visual Studio projects
   single: Visual Studio ; converting to CMake
   single: Visual Studio ; file groups
   single: Visual Studio ; header files
   single: Windows ; executables
   single: WinMain

Converting Windows Based Workspaces
===================================

To convert a Visual Studio solution to CMake involves a few steps. First you 
will need to create a CMakeLists file at the top of your source code 
directory. As always, this file should start with 
:command:`cmake_minimum_required` and :command:`project` command that 
defines the name of the CMake project. This will become the name of the 
resulting Visual Studio solution. Next, add all of your source files into 
CMake variables. For large projects that have multiple directories, create a 
CMakeLists file in each directory as described in the section on source 
directory structures at the beginning of this chapter. You will then add 
your libraries and executables using :command:`add_library` and 
:command:`add_executable`. By default, :command:`add_executable` assumes 
that your executable is a console application. Adding the ``WIN32`` argument 
to :command:`add_executable` indicates that it is a Windows application 
(using WinMain instead of main).

There are a few nice features that Visual Studio supports and CMake
can take advantage of. One is support for class browsing. Typically in
CMake, only source files are added to a target, not header files. If
you add header files to a target, they will show up in the workspace
and then you will be able to browse them as usual. Visual Studio also
supports the notion of groups of files. By default, CMake creates
groups for source files and header files. Using the :command:`source_group`
command, you can create your own groups and assign files to them. If
you have any custom build steps in your workspace, these can be added
to your CMakeLists files using the :command:`add_custom_command`
command. Custom targets (Utility Targets) in Visual Studio can be
added with the :command:`add_custom_target` command.
