Package | Class | Tree | Deprecated | Index | Help
PREV CLASS NEXT CLASS | FRAMES NO FRAMES
SUMMARY: NESTED | FIELD | CONSTR | METHOD | DETAIL: FIELD | CONSTR | METHOD

## org.libjpegturbo.turbojpeg
Class TJ

    java.lang.Object
      org.libjpegturbo.turbojpeg.TJ

    public final class TJ

extends java.lang.Object

TurboJPEG utility class (cannot be instantiated)

Field Summary
`static int` | `FLAG_ACCURATEDCT` Use the most accurate DCT/IDCT algorithm available in the underlying codec.
`static int` | `FLAG_BOTTOMUP` The uncompressed source/destination image is stored in bottom-up (Windows, OpenGL) order, not top-down (X11) order.
`static int` | `FLAG_FASTDCT` Use the fastest DCT/IDCT algorithm available in the underlying codec.
`static int` | `FLAG_FASTUPSAMPLE` When decompressing an image that was compressed using chrominance subsampling, use the fastest chrominance upsampling algorithm available in the underlying codec.
`static int` | `FLAG_FORCEMMX` Turn off CPU auto-detection and force TurboJPEG to use MMX code (if the underlying codec supports it.)
`static int` | `FLAG_FORCESSE` Turn off CPU auto-detection and force TurboJPEG to use SSE code (if the underlying codec supports it.)
`static int` | `FLAG_FORCESSE2` Turn off CPU auto-detection and force TurboJPEG to use SSE2 code (if the underlying codec supports it.)
`static int` | `FLAG_FORCESSE3` Turn off CPU auto-detection and force TurboJPEG to use SSE3 code (if the underlying codec supports it.)
`static int` | `NUMPF` The number of pixel formats
`static int` | `NUMSAMP` The number of chrominance subsampling options
`static int` | `PF_ABGR` ABGR pixel format.
`static int` | `PF_ARGB` ARGB pixel format.
`static int` | `PF_BGR` BGR pixel format.
`static int` | `PF_BGRA` BGRA pixel format.
`static int` | `PF_BGRX` BGRX pixel format.
`static int` | `PF_GRAY` Grayscale pixel format.
`static int` | `PF_RGB` RGB pixel format.
`static int` | `PF_RGBA` RGBA pixel format.
`static int` | `PF_RGBX` RGBX pixel format.
`static int` | `PF_XBGR` XBGR pixel format.
`static int` | `PF_XRGB` XRGB pixel format.
`static int` | `SAMP_420` 4:2:0 chrominance subsampling.
`static int` | `SAMP_422` 4:2:2 chrominance subsampling.
`static int` | `SAMP_440` 4:4:0 chrominance subsampling.
`static int` | `SAMP_444` 4:4:4 chrominance subsampling (no chrominance subsampling).
`static int` | `SAMP_GRAY` Grayscale.

Constructor Summary
`TJ()`

Method Summary
`static int` | `bufSize(int width, int height, int jpegSubsamp)` Returns the maximum size of the buffer (in bytes) required to hold a JPEG image with the given width, height, and level of chrominance subsampling.
`static int` | `bufSizeYUV(int width, int height, int subsamp)` Returns the size of the buffer (in bytes) required to hold a YUV planar image with the given width, height, and level of chrominance subsampling.
`static int` | `getBlueOffset(int pixelFormat)` For the given pixel format, returns the number of bytes that the blue component is offset from the start of the pixel.
`static int` | `getGreenOffset(int pixelFormat)` For the given pixel format, returns the number of bytes that the green component is offset from the start of the pixel.
`static int` | `getMCUHeight(int subsamp)` Returns the MCU block height for the given level of chrominance subsampling.
`static int` | `getMCUWidth(int subsamp)` Returns the MCU block width for the given level of chrominance subsampling.
`static int` | `getPixelSize(int pixelFormat)` Returns the pixel size (in bytes) for the given pixel format.
`static int` | `getRedOffset(int pixelFormat)` For the given pixel format, returns the number of bytes that the red component is offset from the start of the pixel.
`static TJScalingFactor[]` | `getScalingFactors()` Returns a list of fractional scaling factors that the JPEG decompressor in this implementation of TurboJPEG supports.

Methods inherited from class java.lang.Object
`clone, equals, finalize, getClass, hashCode, notify, notifyAll, toString, wait, wait, wait`

Field Detail

### NUMSAMP

    public static final int NUMSAMP

  The number of chrominance subsampling options

  See Also:
    Constant Field Values

### SAMP_444

    public static final int SAMP_444

  4:4:4 chrominance subsampling (no chrominance subsampling). The JPEG or YUV image will contain one chrominance component for every pixel in the source image.

  See Also:
    Constant Field Values

### SAMP_422

    public static final int SAMP_422

  4:2:2 chrominance subsampling. The JPEG or YUV image will contain one chrominance component for every 2x1 block of pixels in the source image.

  See Also:
    Constant Field Values

### SAMP_420

    public static final int SAMP_420

  4:2:0 chrominance subsampling. The JPEG or YUV image will contain one chrominance component for every 2x2 block of pixels in the source image.

  See Also:
    Constant Field Values

### SAMP_GRAY

    public static final int SAMP_GRAY

  Grayscale. The JPEG or YUV image will contain no chrominance components.

  See Also:
    Constant Field Values

### SAMP_440

    public static final int SAMP_440

  4:4:0 chrominance subsampling. The JPEG or YUV image will contain one chrominance component for every 1x2 block of pixels in the source image.

  See Also:
    Constant Field Values

### NUMPF

    public static final int NUMPF

  The number of pixel formats

  See Also:
    Constant Field Values

### PF_RGB

    public static final int PF_RGB

  RGB pixel format. The red, green, and blue components in the image are stored in 3-byte pixels in the order R, G, B from lowest to highest byte address within each pixel.

  See Also:
    Constant Field Values

### PF_BGR

    public static final int PF_BGR

  BGR pixel format. The red, green, and blue components in the image are stored in 3-byte pixels in the order B, G, R from lowest to highest byte address within each pixel.

  See Also:
    Constant Field Values

### PF_RGBX

    public static final int PF_RGBX

  RGBX pixel format. The red, green, and blue components in the image are stored in 4-byte pixels in the order R, G, B from lowest to highest byte address within each pixel. The X component is ignored when compressing and undefined when decompressing.

  See Also:
    Constant Field Values

### PF_BGRX

    public static final int PF_BGRX

  BGRX pixel format. The red, green, and blue components in the image are stored in 4-byte pixels in the order B, G, R from lowest to highest byte address within each pixel. The X component is ignored when compressing and undefined when decompressing.

  See Also:
    Constant Field Values

### PF_XBGR

    public static final int PF_XBGR

  XBGR pixel format. The red, green, and blue components in the image are stored in 4-byte pixels in the order R, G, B from highest to lowest byte address within each pixel. The X component is ignored when compressing and undefined when decompressing.

  See Also:
    Constant Field Values

### PF_XRGB

    public static final int PF_XRGB

  XRGB pixel format. The red, green, and blue components in the image are stored in 4-byte pixels in the order B, G, R from highest to lowest byte address within each pixel. The X component is ignored when compressing and undefined when decompressing.

  See Also:
    Constant Field Values

### PF_GRAY

    public static final int PF_GRAY

  Grayscale pixel format. Each 1-byte pixel represents a luminance (brightness) level from 0 to 255.

  See Also:
    Constant Field Values

### PF_RGBA

    public static final int PF_RGBA

  RGBA pixel format. This is the same as `PF_RGBX`, except that when decompressing, the X byte is guaranteed to be 0xFF, which can be interpreted as an opaque alpha channel.

  See Also:
    Constant Field Values

### PF_BGRA

    public static final int PF_BGRA

  BGRA pixel format. This is the same as `PF_BGRX`, except that when decompressing, the X byte is guaranteed to be 0xFF, which can be interpreted as an opaque alpha channel.

  See Also:
    Constant Field Values

### PF_ABGR

    public static final int PF_ABGR

  ABGR pixel format. This is the same as `PF_XBGR`, except that when decompressing, the X byte is guaranteed to be 0xFF, which can be interpreted as an opaque alpha channel.

  See Also:
    Constant Field Values

### PF_ARGB

    public static final int PF_ARGB

  ARGB pixel format. This is the same as `PF_XRGB`, except that when decompressing, the X byte is guaranteed to be 0xFF, which can be interpreted as an opaque alpha channel.

  See Also:
    Constant Field Values

### FLAG_BOTTOMUP

    public static final int FLAG_BOTTOMUP

  The uncompressed source/destination image is stored in bottom-up (Windows, OpenGL) order, not top-down (X11) order.

  See Also:
    Constant Field Values

### FLAG_FORCEMMX

    public static final int FLAG_FORCEMMX

  Turn off CPU auto-detection and force TurboJPEG to use MMX code (if the underlying codec supports it.)

  See Also:
    Constant Field Values

### FLAG_FORCESSE

    public static final int FLAG_FORCESSE

  Turn off CPU auto-detection and force TurboJPEG to use SSE code (if the underlying codec supports it.)

  See Also:
    Constant Field Values

### FLAG_FORCESSE2

    public static final int FLAG_FORCESSE2

  Turn off CPU auto-detection and force TurboJPEG to use SSE2 code (if the underlying codec supports it.)

  See Also:
    Constant Field Values

### FLAG_FORCESSE3

    public static final int FLAG_FORCESSE3

  Turn off CPU auto-detection and force TurboJPEG to use SSE3 code (if the underlying codec supports it.)

  See Also:
    Constant Field Values

### FLAG_FASTUPSAMPLE

    public static final int FLAG_FASTUPSAMPLE

  When decompressing an image that was compressed using chrominance subsampling, use the fastest chrominance upsampling algorithm available in the underlying codec. The default is to use smooth upsampling, which creates a smooth transition between neighboring chrominance components in order to reduce upsampling artifacts in the decompressed image.

  See Also:
    Constant Field Values

### FLAG_FASTDCT

    public static final int FLAG_FASTDCT

  Use the fastest DCT/IDCT algorithm available in the underlying codec. The default if this flag is not specified is implementation-specific. The libjpeg implementation, for example, uses the fast algorithm by default when compressing, because this has been shown to have only a very slight effect on accuracy, but it uses the accurate algorithm when decompressing, because this has been shown to have a larger effect.

  See Also:
    Constant Field Values

### FLAG_ACCURATEDCT

    public static final int FLAG_ACCURATEDCT

  Use the most accurate DCT/IDCT algorithm available in the underlying codec. The default if this flag is not specified is implementation-specific. The libjpeg implementation, for example, uses the fast algorithm by default when compressing, because this has been shown to have only a very slight effect on accuracy, but it uses the accurate algorithm when decompressing, because this has been shown to have a larger effect.

  See Also:
    Constant Field Values

Constructor Detail

### TJ

    public TJ()

Method Detail

### getMCUWidth

    public static int getMCUWidth(int subsamp)
                           throws java.lang.Exception

  Returns the MCU block width for the given level of chrominance subsampling.

  Parameters:
    `subsamp` - the level of chrominance subsampling (one of `SAMP_*`)
  Returns:
    the MCU block width for the given level of chrominance subsampling
  Throws:
    `java.lang.Exception`

### getMCUHeight

    public static int getMCUHeight(int subsamp)
                            throws java.lang.Exception

  Returns the MCU block height for the given level of chrominance subsampling.

  Parameters:
    `subsamp` - the level of chrominance subsampling (one of `SAMP_*`)
  Returns:
    the MCU block height for the given level of chrominance subsampling
  Throws:
    `java.lang.Exception`

### getPixelSize

    public static int getPixelSize(int pixelFormat)
                            throws java.lang.Exception

  Returns the pixel size (in bytes) for the given pixel format.

  Parameters:
    `pixelFormat` - the pixel format (one of `PF_*`)
  Returns:
    the pixel size (in bytes) for the given pixel format
  Throws:
    `java.lang.Exception`

### getRedOffset

    public static int getRedOffset(int pixelFormat)
                            throws java.lang.Exception

  For the given pixel format, returns the number of bytes that the red component is offset from the start of the pixel. For instance, if a pixel of format `TJ.PF_BGRX` is stored in `char pixel[]`, then the red component will be `pixel[TJ.getRedOffset(TJ.PF_BGRX)]`.

  Parameters:
    `pixelFormat` - the pixel format (one of `PF_*`)
  Returns:
    the red offset for the given pixel format
  Throws:
    `java.lang.Exception`

### getGreenOffset

    public static int getGreenOffset(int pixelFormat)
                              throws java.lang.Exception

  For the given pixel format, returns the number of bytes that the green component is offset from the start of the pixel. For instance, if a pixel of format `TJ.PF_BGRX` is stored in `char pixel[]`, then the green component will be `pixel[TJ.getGreenOffset(TJ.PF_BGRX)]`.

  Parameters:
    `pixelFormat` - the pixel format (one of `PF_*`)
  Returns:
    the green offset for the given pixel format
  Throws:
    `java.lang.Exception`

### getBlueOffset

    public static int getBlueOffset(int pixelFormat)
                             throws java.lang.Exception

  For the given pixel format, returns the number of bytes that the blue component is offset from the start of the pixel. For instance, if a pixel of format `TJ.PF_BGRX` is stored in `char pixel[]`, then the blue component will be `pixel[TJ.getBlueOffset(TJ.PF_BGRX)]`.

  Parameters:
    `pixelFormat` - the pixel format (one of `PF_*`)
  Returns:
    the blue offset for the given pixel format
  Throws:
    `java.lang.Exception`

### bufSize

    public static int bufSize(int width,
                              int height,
                              int jpegSubsamp)
                       throws java.lang.Exception

  Returns the maximum size of the buffer (in bytes) required to hold a JPEG image with the given width, height, and level of chrominance subsampling.

  Parameters:
    `width` - the width (in pixels) of the JPEG image
    `height` - the height (in pixels) of the JPEG image
    `jpegSubsamp` - the level of chrominance subsampling to be used when generating the JPEG image (one of `TJ.SAMP_*`)
  Returns:
    the maximum size of the buffer (in bytes) required to hold a JPEG image with the given width, height, and level of chrominance subsampling
  Throws:
    `java.lang.Exception`

### bufSizeYUV

    public static int bufSizeYUV(int width,
                                 int height,
                                 int subsamp)
                          throws java.lang.Exception

  Returns the size of the buffer (in bytes) required to hold a YUV planar image with the given width, height, and level of chrominance subsampling.

  Parameters:
    `width` - the width (in pixels) of the YUV image
    `height` - the height (in pixels) of the YUV image
    `subsamp` - the level of chrominance subsampling used in the YUV image (one of `TJ.SAMP_*`)
  Returns:
    the size of the buffer (in bytes) required to hold a YUV planar image with the given width, height, and level of chrominance subsampling
  Throws:
    `java.lang.Exception`

### getScalingFactors

    public static TJScalingFactor[] getScalingFactors()
                                               throws java.lang.Exception

  Returns a list of fractional scaling factors that the JPEG decompressor in this implementation of TurboJPEG supports.

  Returns:
    a list of fractional scaling factors that the JPEG decompressor in this implementation of TurboJPEG supports
  Throws:
    `java.lang.Exception`

Package | Class | Tree | Deprecated | Index | Help
PREV CLASS NEXT CLASS | FRAMES NO FRAMES
SUMMARY: NESTED | FIELD | CONSTR | METHOD | DETAIL: FIELD | CONSTR | METHOD