// Generated by CMB
ModelInfo:
{
  File: pillboxwg.ncdf

  BoundaryCondition: {
    Absorbing: 3,4
    Exterior: 5,6
    Magnetic: 1,2
  }
}

FiniteElement:
{
  Order: 1
  CurvedSurfaces: on
}

CheckPoint:
{
  Action: restart
  Ntimesteps: 1000
}

LoadingInfo:
{

  Bunch:
  {
  Type: Gaussian
  Sigma: 0.010000
  Number of sigmas: 5
  Charge: 1e-12
  }
  SymmetryFactor: 4.0
  StartPoint: 0, 0, -0.075
  Direction: 0, 0, 1
  BoundaryID: 3
}

TimeStepping:
{
  MaximumTime: 5e-09
  DT: 2e-12
}

Monitor:
{
  Type: ModeVoltage
  Name: mode-voltage
  Port: {
    ReferenceNumber: 6
    ESolver: {
      Type: Numerical2D
      NumberOfModes: 1
      Frequency: 1e+09
      Tolerance: 1e-15
      MaxIterations: 1000
    }
  }
}

Monitor:
{
  Type: Power
  Name: power-monitor
  TimeStart: 0.0
  ReferenceNumber: 5
}

Monitor:
{
  Type: Volume
  Name: mymon
  TimeStart: 0.0
  TimeEnd: 5e-09
  TimeStep: 1e-10
}

Monitor:
{
  Type: WakeField
  Name: wakefield
  StartContour: -0.075
  EndContour: 0.075
  Smax: 1.4
}

LinearSolver:
{
  Solver: MUMPS
}
