### Description

This example shows the isoparametric cells supported by the VTK. These cells are nonlinear and contain one or more mid-side vertices. Isoparametric elements are typically used in [finite element analysis](https://en.wikipedia.org/wiki/Finite_element_method).  The term isoparametric is derived from the use of the same shape functions (or interpolation functions)  to define the element's geometric shape as are used to define the displacements within the element.

This example illustrates each cell's representation using its parametric coordinates (pcoords) as the vertices of the cell. In practice, the vertices will correspond to physical points in a finite element model. Use vtkTessellatorFilter to better see the shape of the cell. See for example, [QuadraticHexahedronDemo](../QuadraticHexahedronDemo) and [QuadraticTetraDemo](../QuadraticTetraDemo).
