# EllipticalCylinderDemo

VTKExamples/Python/GeometricObjects/EllipticalCylinderDemo

### Description

The example shows the vtkPolyLine that forms the base of the elliptical cylinder and an oriented arrow that represents the vector that vtkLinearExtrusionFilter uses to create the cylinder. The example takes an optional triple that defines the vector for the filter. The length of the vector is the height of the cylinder.

Other Languages

See (Cxx)

### Code

EllipticalCylinderDemo.py

    #!/usr/bin/env python
    # -*- coding: utf-8 -*-

    import math

    import vtk

    def main():
        nx, ny, nz = get_program_parameters()
        colors = vtk.vtkNamedColors()

        angle = 0
        r1 = 50
        r2 = 30
        centerX = 10.0
        centerY = 5.0

        points = vtk.vtkPoints()
        idx = 0
        while angle <= 2.0 * vtk.vtkMath.Pi() + (vtk.vtkMath.Pi() / 60.0):
            points.InsertNextPoint(r1 * math.cos(angle) + centerX,
                                   r2 * math.sin(angle) + centerY,
                                   0.0)
            angle = angle + (vtk.vtkMath.Pi() / 60.0)
            idx += 1

        line = vtk.vtkPolyLine()
        line.GetPointIds().SetNumberOfIds(idx)
        for i in range(0, idx):
            line.GetPointIds().SetId(i, i)

        lines = vtk.vtkCellArray()
        lines.InsertNextCell(line)

        polyData = vtk.vtkPolyData()
        polyData.SetPoints(points)
        polyData.SetLines(lines)

        extrude = vtk.vtkLinearExtrusionFilter()
        extrude.SetInputData(polyData)
        extrude.SetExtrusionTypeToNormalExtrusion()
        extrude.SetVector(nx, ny, nz)
        extrude.Update()

        # Create an oriented arrow
        startPoint = [0.0] * 3
        endPoint = [0.0] * 3
        startPoint[0] = centerX
        startPoint[1] = centerY
        startPoint[2] = 0.0
        endPoint[0] = startPoint[0] + extrude.GetVector()[0]
        endPoint[1] = startPoint[1] + extrude.GetVector()[1]
        endPoint[2] = startPoint[2] + extrude.GetVector()[2]

        # Compute a basis
        normalizedX = [0.0] * 3
        normalizedY = [0.0] * 3
        normalizedZ = [0.0] * 3

        # The X axis is a vector from start to end
        vtk.vtkMath.Subtract(endPoint, startPoint, normalizedX)
        length = vtk.vtkMath.Norm(normalizedX)
        vtk.vtkMath.Normalize(normalizedX)

        # The Z axis is an arbitrary vector cross X
        arbitrary = [0.0] * 3
        arbitrary[0] = vtk.vtkMath.Random(-10, 10)
        arbitrary[1] = vtk.vtkMath.Random(-10, 10)
        arbitrary[2] = vtk.vtkMath.Random(-10, 10)
        vtk.vtkMath.Cross(normalizedX, arbitrary, normalizedZ)
        vtk.vtkMath.Normalize(normalizedZ)

        # The Y axis is Z cross X
        vtk.vtkMath.Cross(normalizedZ, normalizedX, normalizedY)
        matrix = vtk.vtkMatrix4x4()

        # Create the direction cosine matrix
        matrix.Identity()
        for i in range(0, 3):
            matrix.SetElement(i, 0, normalizedX[i])
            matrix.SetElement(i, 1, normalizedY[i])
            matrix.SetElement(i, 2, normalizedZ[i])

        # Apply the transforms
        transform = vtk.vtkTransform()
        transform.Translate(startPoint)
        transform.Concatenate(matrix)
        transform.Scale(length, length, length)

        arrowSource = vtk.vtkArrowSource()
        arrowSource.SetTipResolution(31)
        arrowSource.SetShaftResolution(21)

        # Transform the polydata
        transformPD = vtk.vtkTransformPolyDataFilter()
        transformPD.SetTransform(transform)
        transformPD.SetInputConnection(arrowSource.GetOutputPort())

        # Create a mapper and actor for the arrow
        arrowMapper = vtk.vtkPolyDataMapper()
        arrowMapper.SetInputConnection(transformPD.GetOutputPort())

        arrowActor = vtk.vtkActor()
        arrowActor.SetMapper(arrowMapper)
        arrowActor.GetProperty().SetColor(colors.GetColor3d("Tomato"))

        tubes = vtk.vtkTubeFilter()
        tubes.SetInputData(polyData)
        tubes.SetRadius(2.0)
        tubes.SetNumberOfSides(21)

        lineMapper = vtk.vtkPolyDataMapper()
        lineMapper.SetInputConnection(tubes.GetOutputPort())

        lineActor = vtk.vtkActor()
        lineActor.SetMapper(lineMapper)
        lineActor.GetProperty().SetColor(colors.GetColor3d("Peacock"))

        mapper = vtk.vtkPolyDataMapper()
        mapper.SetInputConnection(extrude.GetOutputPort())

        actor = vtk.vtkActor()
        actor.SetMapper(mapper)
        actor.GetProperty().SetColor(colors.GetColor3d("Banana"))
        actor.GetProperty().SetOpacity(.7)

        ren = vtk.vtkRenderer()
        ren.SetBackground(colors.GetColor3d("SlateGray"))
        ren.AddActor(actor)
        ren.AddActor(lineActor)
        ren.AddActor(arrowActor)

        renWin = vtk.vtkRenderWindow()
        renWin.SetWindowName("Elliptical Cylinder Demo")
        renWin.AddRenderer(ren)
        renWin.SetSize(600, 600)

        iren = vtk.vtkRenderWindowInteractor()
        iren.SetRenderWindow(renWin)

        style = vtk.vtkInteractorStyleTrackballCamera()
        iren.SetInteractorStyle(style)

        camera = vtk.vtkCamera()
        camera.SetPosition(0, 1, 0)
        camera.SetFocalPoint(0, 0, 0)
        camera.SetViewUp(0, 0, 1)
        camera.Azimuth(30)
        camera.Elevation(30)

        ren.SetActiveCamera(camera)
        ren.ResetCamera()
        ren.ResetCameraClippingRange()

        renWin.Render()
        iren.Start()

    def get_program_parameters():
        import argparse
        description = 'Elliptical Cylinder Demo.'
        epilogue = '''
    The example shows the vtkPolyLine that forms the base of the elliptical cylinder
     and an oriented arrow that represents the vector that vtkLinearExtrusionFilter
     uses to create the cylinder.
    The example takes an optional triple that defines the vector for the filter.
    The length of the vector is the height of the cylinder.
        '''
        parser = argparse.ArgumentParser(description=description, epilog=epilogue,
                                         formatter_class=argparse.RawDescriptionHelpFormatter)
        parser.add_argument('-nx', nargs='?', const=0.0, default=0.0, type=float)
        parser.add_argument('-ny', nargs='?', const=0.0, default=0.0, type=float)
        parser.add_argument('-nz', nargs='?', const=100.0, default=100.0, type=float)
        args = parser.parse_args()
        return args.nx, args.ny, args.nz

    if __name__ == '__main__':
        main()