OP HT
OP GW
OP TRN 0
IP NIT 9  ! Maximum number of non-linear iterations
IP NTL 1e-10 ! Non-Linear absolute tolerance
IP ITL 1e-05  ! Non-Linear incremental tolerance
IP MIT 500  ! Maximum number of linear iterations
OP BLK 8  ! Number of blocks per processor for pre-conditioner
OP PRE 0  ! Preconditioner type
OP INC 1  ! Incremental memory size
TC T0 200 1   ! Starting time of the simulation
TC TF 200 1  ! Final time of the simulation
TC IDT 1 ! The XY Series that will control the time step size
OC 1  ! Output, the XY series that sets the time levels that are printed out during the simulations
OC ADP  ! Print out the adapted mesh
DB FLW 1 3 ! Dirichlet boundary condition for flow nodalbc
NB HFX 2 4 ! Heat Flux boundary condition for temperature facebc
! material -- realmaterial
MP POR 1 0.5  ! Porosity
MP K   1 1 1 1 0 0 0  ! Hydraulic conductivity
MP SAT 1 3  ! Pressure saturation curve, XY series number
MP KR  1 4  ! Pressure relative conductivity curve, XY series number
MP SS  1 1e-06  ! Specific storage
MP SHS 1 0.0001  ! Specific heat of solids
MP SGS 1 2.65  ! Specific gravity of solids
MP ALB 1 0.3  ! Albedo
MP EMS 1 0.8  ! Bulk emissivity
MP THK 1 1 1 1 0 0 0  ! Thermal conductivity, Units = (W)/(m K) 
MP TOR 1 0.7 ! Tortuosity
MP DPL 1 1  ! Longitudinal dispersivity
MP DPT 1 0.1  ! Transverse dispersivity
MP ML  1 0  ! Refinement levels
MP FRT 1 1  ! Refinement Tolerance
MP MID 1 13
OP SOC 200 300  ! Socket numbers for adh/raycaster communication (in/out for adh)
MP G   1.27202e+08  ! Gravity, (m)/(hr^2)
MP SHW 4.1813  ! Specific heat of water, Units = (W-hr)/(g K)
MP SHG 1.0035  !  Specific heat of gas, Units = (W-hr)/(g K)
MP SGW 1  ! Specific gravity of water
MP SGG 0.001  ! Specific gravity of gas
MP TKW 0.58  ! Thermal conductivity of water, Units = (W)/(m K)
MP TKG 0.024  ! Thermal conductivity of gas, Units = (W)/(m K)
MP RHO 1e+06  ! Reference density, g/m^3
MP VIS 1e-05  ! Reference viscosity, Units = ?
! function -- time
XYT 1 1.0e20
XY1 1 9 0 0 0 0
2 2
3 3
4 4
5 5
6 6
7 7
8 8
9 9
10 10

! function -- notused
XY1 2 9 0 0 0 0
2 2
3 3
4 4
6 6
7 7
8 8
9 9
10 10
100 0

! function -- function2
XY1 3 10 0 0 0 0
0 0
0 0
0 0
0 0
0 0
0 0
0 0
0 0
0 0
0 0

! function -- function3
XY1 4 10 0 0 0 0
0 0
0 0
0 0
0 0
0 0
0 0
0 0
0 0
0 0
0 0

NDS 8 1
NDS 9 1
NDS 7 1
NDS 5 1
NDS 6 1
NDS 10 1
NDS 12 1
NDS 11 1
FCS 8 3 2
FCS 9 1 2
END
